Please run the driver on WinPAC and intall it.

Notes: 
	1. The OS of WP8x4x/WP8x3x && Touch driver
		           OS			               Touch driver
                           V1410 or earlier                    Egalax_Serial_TOUCH_V20081027.CAB
                           V1410 or earlier                    Egalax_USB_TOUCH_V20081107.CAB
                           V1410 or earlier                    ELO_Serial_TOUCH_V20081027.CAB
                           V1410 or earlier                    ELO_USB_TOUCH_V20081118.CAB
                           V1410 or earlier                    PenMount_Serial_TOUCH_V20081117.CAB
                           V1410 or earlier                    PenMount_USB_TOUCH_V20081023.CAB
                    ----------------------------------------------------------------------------------------------------------		
                           V1420 or later                       Egalax_Serial_TOUCH_V20100507.CAB
                           V1420 or later                       Egalax_USB_TOUCH_V20100507.CAB
                           V1420 or later                       ELO_Serial_TOUCH_V20100507.CAB
                           V1420 or later                       ELO_USB_TOUCH_V20100506.CAB
                           V1420 or later                       PenMount_Serial_TOUCH_V20091102.CAB
                           V1420 or later                       PenMount_Serial_TOUCH_V20100824(PM6000R).CAB
                           V1420 or later                       PenMount_USB_TOUCH_V20100507.CAB		
                    -----------------------------------------------------------------------------------------------------------
                           V1710/V1600 or later                 PM6000_Serial_TOUCH_V20130903.CAB
                           V1710/V1600 or later                 PenMount_Serial_TOUCH_V20130904(PM6000R).CAB
                           V1710/V1600 or later                 PenMount_Serial_TOUCH_V20130904.CAB
                        
	2. The serial touch panel can be attached on either of the COM1/COM3/COM4 
        on WinPAC and the SetCOM.exe is provided to change the COM port number for 
        the touch panel driver.
	3. The default COM port of all serial touch panel driver is set on COM4.

Installation document:
	CD\napdos\wp-8x4x_ce50\Document\How_To\General IO Expansion
                  
	1. w1-004-01_how_to_set_up_an_Egalax_USB_touch_panel_english.pdf		      
	2. w1-004-02_how_to_set_up_an_ELO_USB_touch_panel_english.pdf
	3. w1-004-03_how_to_set_up_a_Penmount_USB_touch_panel_english.pdf
	4. w1-004-04_how_to_set_up_an_Egalax_serial_touch_panel_english.pdf
	5. w1-004-05_how_to_set_up_an_ELO_serial_touch_panel_english.pdf
	6. w1-004-06_how_to_set_up_a_Penmoumt_serial_touch_panel_english.pdf

Calibartion document:
	CD\napdos\wp-8x4x_ce50\Document\How_To\General IO Expansion

	1. w1-005-01_how_to_calibrate_an_Egalax_USB_touch_panel_english.pdf
	2. w1-005-02_how_to_calibrate_an_ELO_USB_touch_panel_english.pdf
	3. w1-005-03_how_to_calibrate_a_Penmount_USB_touch_panel_english.pdf
	4. w1-005-04_how_to_calibrate_an_Egalax_serial_touch_panel_english.pdf
	5. w1-005-05_how_to_calibrate_an_ELO_serial_touch_panel_english.pdf
	6. w1-005-06_how_to_calibrate_a_Penmoumt_serial_touch_panel_english.pdf
========================================================================

== External Deviec Driver ==
-------------------------------------------------------------------------------------------------------------------------------

PenMount:

For ADP-1080T-U(Aplex), 3M DynaPro, PenMount, USB Touch Panel
  driver : PenMount_USB_TOUCH_Vyyyymmdd.CAB
  (ADP-1080T-U : http://www.icpdas.com/products/HMI/touch_lcd/adp-1080t-r_u.htm)

For ADP-1080T-R(Aplex), 3M DynaPro, PenMount, RS-232 Touch Panel
  driver : PenMount_Serial_TOUCH_Vyyyymmdd.CAB
  (ADP-1080T-R : http://www.icpdas.com/products/HMI/touch_lcd/adp-1080t-r_u.htm)

For AFL-08MH/T-R-R11
  driver: PM6000_Serial_TOUCH_Vyyyymmdd.CAB

For TP-4100/TPM-4100
  Driver: PenMount_Serial_TOUCH_Vyyyymmdd(PM6000R).CAB

Note: Please use the laster version driver. If you have and problems, please email to ICPDAS.
-------------------------------------------------------------------------------------------------------------------------------
Egalax:

For GA-700YY-USB, 7" USB Touch Panel
  driver : Egalax_USB_TOUCH_Vyyyymmdd.CAB
  (GA-700YY-USB : http://www.icpdas.com/products/HMI/touch_lcd/ga-700yy.htm)

For GA-700YY-UOM, 7" RS-232 Touch Panel and AFL-17M/TR-R11 
  driver : Egalax_Serial_TOUCH_Vyyyymmdd.CAB
  (GA-700YY-UOM : http://www.icpdas.com/products/HMI/touch_lcd/ga-700yy.htm)
-------------------------------------------------------------------------------------------------------------------------------
ELO:

For ELO USB Touch Panel
  driver : ELO_USB_TOUCH_Vyyyymmdd.CAB
 
For ELO RS-232 Touch Panel
  driver : ELO_Serial_TOUCH_Vyyyymmdd.CAB
-------------------------------------------------------------------------------------------------------------------------------

==End ==









  